**Photoionization/Flame Ionization Detector (PID/FID) Calibration Record**

|  |
| --- |
| **Date:** **Calibrated By:** |
| **Equipment Manufacturer:** |
| **Model:** **Serial Number:** |
| **Lamp Intensity (eV):** |
| **Battery Fully Charged: Yes No** |
| **Temperature (°F):** **Relative Humidity (%):**  |
| **Calibration Location:** |
| **Fresh or Zero Air Calibration: Yes No**  |

|  |
| --- |
| **CALIBRATION GASES** |
| **Manufacturer****(if applicable)** | **Calibration/Span Gas** | **Shelf-Life Specified on Cylinder** **(if applicable)** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |
| --- |
| **EQUIPMENT CALIBRATION** |
| **Calibration/Span Gas****[e.g., isobutylene, methane, other (specify)]** | **Instrument Reading****(units)** | **Calibration/Span Gas****Concentration****(span value)** | **Instrument Adjustment****(span value change)****(Yes/No/Self-adjusts\*)** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
| \* Specify "self-adjusts" when the equipment sets its own sensitivity to the calibration gas. **Comments:** |