**Photoionization/Flame Ionization Detector (PID/FID) Calibration Record**

|  |
| --- |
| **Date:** **Calibrated By:** |
| **Equipment Manufacturer:** |
| **Model:** **Serial Number:** |
| **Lamp Intensity (eV):** |
| **Battery Fully Charged: Yes No** |
| **Temperature (°F):** **Relative Humidity (%):** |
| **Calibration Location:** |
| **Fresh or Zero Air Calibration: Yes No** |

|  |  |  |
| --- | --- | --- |
| **CALIBRATION GASES** | | |
| **Manufacturer**  **(if applicable)** | **Calibration/Span Gas** | **Shelf-Life Specified on Cylinder**  **(if applicable)** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **EQUIPMENT CALIBRATION** | | | |
| **Calibration/Span Gas**  **[e.g., isobutylene, methane, other (specify)]** | **Instrument Reading**  **(units)** | **Calibration/Span Gas**  **Concentration**  **(span value)** | **Instrument Adjustment**  **(span value change)**  **(Yes/No/Self-adjusts\*)** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
| \* Specify "self-adjusts" when the equipment sets its own sensitivity to the calibration gas.  **Comments:** | | | |